Delhi Jal Board — STP Utilisation Analysis
Source: RTI Act 2005, ID No. 47, dated 08.05.2026 | Analysis updated with all RTI responses
 
Aggregate Summary
	Metric
	Value

	Total STPs identified
	32

	STPs at 100% utilisation
	10 (31.3% of total)

	STPs overloaded (>100%)
	5 (15.6% of total)

	STPs underutilised (<100%)
	17 (53.1% of total)

	Total Installed Capacity (MGD)
	713.6 MGD

	Total Utilised Capacity (MGD)
	601.51 MGD

	Overall Utilisation Rate
	84.3%

	New STPs / upgrades (last 5 yrs)
	Yamuna Vihar Ph-II upgraded 2025; Sonia Vihar commissioned 2024; Keshopur Ph-III upgraded 40→60 MGD; Rohini STP +10 MGD (Rs 37.50 Cr)

	Dual-zone conflicts identified
	2 (Yamuna Vihar: SE-I vs EE-XIII; Rithala: EE-XII vs EE-IX)

	Plants with NIL O&M (last 5 yrs)
	1 (Rithala Ph-I — under rehabilitation despite 101.7% loading)


 
NOTE: Kondli Ph I-IV and Chilla STP (EE-SDW-IV) — RTI response withheld as 'bulky'; utilisation claimed 100% by division but no granular data provided. Figures above use division claim. Independent verification not possible from RTI alone.
 
STP-wise Detail: Installed Capacity, Utilisation, O&M and Remarks
	Zone
	Division
	STP Name
	Installed (MGD)
	Utilised (MGD)
	Rate %
	O&M Expenditure (Last 5 Yrs)
	Capital Cost
	Commissioned
	Anomaly / Remarks

	SE-I
	EE(SDW)-III
	Yamuna Vihar Ph-I
	10
(45 MLD)
	2.20
	22%
	Not disclosed
	—
	Pre-2020
	Severely underutilised. Only 22% capacity used.

	
	
	Yamuna Vihar Ph-II
	15
(68 MLD)
	3.30
	22%
	Not disclosed
	Rs 60.75 Cr (Govt. of India)
	2025 (upgraded +5 MGD)
	Upgraded capacity. Severely underutilised. Only 22% capacity used.

	
	
	Sonia Vihar WWTP
	7.0
(32 MLD)
	0.11
	1.6%
	Not disclosed
	Rs 55.70 Cr (GNCT of Delhi)
	2024
	Brand new plant. Severely underutilised. Only 1.6% capacity used despite full capital expenditure.

	SE-I
	EE(SDW)-XIII
	Yamuna Vihar (25 MGD)
	25
(114 MLD)
	28-29
	112-116%
	FY22: 4.92 Cr | FY23: 4.83 Cr | FY24: 4.86 Cr | FY25: 5.1 Cr | FY26: 2.7 Cr
	—
	2015
	OVERLOADED. Dual-zone conflict: SE-I reports 25 MGD (100%), EE-XIII reports 28-29 MGD actual flow. No CPCB/NGT penalty yet.

	EE(SDW)-IV
	EE(SDW)-IV
	Kondli Ph-I
	10
	10
	100%
	Voluminous — visit office
	—
	Not disclosed
	100% utilised per division claim. Granular data withheld.

	
	
	Kondli Ph-II
	25
	25
	100%
	Voluminous — visit office
	—
	Not disclosed
	100% utilised per division claim. Granular data withheld.

	
	
	Kondli Ph-III
	25
	25
	100%
	Voluminous — visit office
	—
	Not disclosed
	100% utilised per division claim. Granular data withheld.

	
	
	Kondli Ph-IV
	45
	45
	100%
	Voluminous — visit office
	—
	Not disclosed
	100% utilised per division claim. Granular data withheld. RTI obligation not fully met.

	
	
	Chilla STP
	9
	9
	100%
	Voluminous — visit office
	—
	Not disclosed
	100% utilised per division claim. Granular data withheld.

	EE(SDW)-XIV
	EE(SDW)-XIV
	CWG Village Akshardham
	1
(4.55 MLD)
	0.25
	25%
	FY21-26: Rs 83.76 L/yr each year (flat — zero variation; DDA deposit work)
	—
	2010
	DDA deposit work — not DJB-owned. Budget by DDA. Flat O&M across 5 years is suspicious. 75% capacity idle. Meets CPCB/DPCC/NGT norms per RTI.

	EE(SDW)-II
	EE(SDW)-II (Okhla)
	Okhla 124 MGD
	124
(564 MLD)
	100
	81%
	Voluminous — visit office
	Rs 1168 Cr (15% Delhi Govt + 85% Centre)
	2025
	Brand new plant running at only 81%. 24 MGD idle. Parallels Sonia Vihar — massive capital deployed, underutilised from day one.

	
	
	Okhla 30 MGD
	30
(136 MLD)
	13
	43%
	Voluminous — visit office
	—
	Not disclosed
	17 MGD idle. Over 50% unused at established STP.

	
	
	Okhla 16 MGD
	16
(73 MLD)
	7
	44%
	Voluminous — visit office
	—
	Not disclosed
	9 MGD idle. Over 50% unused.

	EE(SDW)-V
	EE(SDW)-V
	Delhi Gate Ph-II
	15
(68 MLD)
	15
	100%
	~Rs 30 L/month
	—
	2016
	Full capacity. No discrepancy. No CPCB/NGT penalty.

	
	
	Delhi Gate Ph-I
	2.2
(10 MLD)
	2.2
	100%
	Maintained by PPCL (third-party)
	—
	1998
	Full capacity. Operated by PPCL. No CPCB/NGT penalty.

	
	
	SNH
	2.2
(10 MLD)
	2.2
	100%
	Maintained by PPCL (third-party)
	—
	1998
	Full capacity. Operated by PPCL. No CPCB/NGT penalty.

	
	
	Ghitorani
	5.0
(23 MLD)
	3
	60%
	~Rs 5.50 L/month
	—
	2015
	2 MGD idle. Moderately underutilised. No CPCB/NGT penalty.

	
	
	Vasant Kunj Ph-I
	2.2
(10 MLD)
	1.75
	80%
	~Rs 2.95 L/month
	—
	1982
	0.45 MGD spare. Oldest STP in dataset. No CPCB/NGT penalty.

	
	
	Vasant Kunj Ph-II
	3
(14 MLD)
	2.10
	70%
	~Rs 1.70 L/month
	—
	2001
	0.9 MGD spare. Moderately underutilised. No CPCB/NGT penalty.

	EE(SDW)-XI
	EE(SDW)-XI
	Mehrauli STP
	5
(23 MLD)
	4.99
	99.8%
	FY21: 49.92 L | FY22: 29.99 L | FY23: 131.19 L | FY24: 79.95 L | FY25: 58.70 L
	—
	2003
	Near-full utilisation. O&M varies significantly (131.19 L in FY23 vs 29.99 L in FY22 — 4x spike, unexplained). No CPCB/NGT penalty.

	EE(SDW)-VI
	EE(SDW)-VI
	Keshopur STP Ph-I
	12
	12.80
	107%
	Withheld — accounts section
	—
	Not disclosed
	OVERLOADED. 12.80 MGD treated vs 12 MGD design. No new STPs commissioned in last 5 yrs. No CPCB/NGT penalty data provided.

	
	
	Keshopur STP Ph-II
	20
	14.12
	70.6%
	Withheld — accounts section
	—
	Not disclosed
	5.88 MGD idle. Moderately underutilised.

	
	
	Keshopur STP Ph-III
	60
	32.17
	53.6%
	Withheld — accounts section
	—
	Pre-2025 (was 40 MGD; upgraded to 60 MGD)
	Capacity upgraded from 40 to 60 MGD before 20.02.2025. Despite upgrade, only 53.6% utilised. 27.83 MGD idle — severe underuse post-upgrade.

	
	
	Najafgarh STP
	5
	4.13
	82.6%
	Withheld — accounts section
	—
	Not disclosed
	0.87 MGD spare. Reasonably utilised.

	
	
	Nilothi STP-II
	20
	20.50
	102.5%
	Withheld — accounts section
	—
	Not disclosed
	OVERLOADED. 0.50 MGD above design capacity. Sewage inflow exceeds treatment capacity.

	EE(SDW)-XII
	EE(SDW)-XII
	Rohini STP
	25
	25
	100%
	FY22: 264.42 L | FY23: 904.25 L | FY24: 7035.00 L | FY25: 1385.87 L | FY26: 4168.61 L | Total alloc FY21-26: Rs 21992.25 L; Expended: Rs 13758.15 L
	Rs 37.50 Cr (upgrade +10 MGD)
	Not disclosed
	100% utilised. Upgraded by 10 MGD. CRITICAL: O&M FY24 = Rs 7035 L (Rs 70.35 Cr) — 5x the next highest year. Massive unexplained spike. Total budget utilisation only 62.5% (13758/21992).

	
	
	Rithala STP (EE-XII claim)
	40
	40
	100%
	Same as above (combined O&M for both STPs)
	—
	Not disclosed
	NOTE: EE-XII claims 100% utilisation. EE-IX reports same plant at 40.69 MGD (101.7%). Dual-zone conflict — see EE-IX row below.

	EE(SDW)-IX
	EE(SDW)-IX
	Rithala Ph-I (EE-IX claim)
	40
	40.69
	101.7%
	NIL for last 5 years (plant under rehabilitation)
	—
	Not disclosed
	OVERLOADED. 40.69 MGD vs 40 MGD design. O&M NIL — plant under rehabilitation. DUAL-ZONE CONFLICT with EE-XII which also claims jurisdiction over Rithala STP at 40 MGD/100%.

	EE(SDW)-VII
	EE(SDW)-VII
	Coronation Pillar NSTP 70 MGD
	70
	67.5
	96.4%
	Not disclosed
	—
	Not disclosed
	Utilisation 60-75 MGD range reported. Midpoint 67.5 MGD used. Near-full capacity.

	
	
	Coronation Pillar NSTP 20 MGD
	20
	22.5
	112.5%
	Not disclosed
	—
	Not disclosed
	OVERLOADED. Utilisation 20-25 MGD range vs 20 MGD design. Midpoint 22.5 used.

	
	
	Coronation Pillar NSTP 10 MGD
	10
	9
	90%
	Not disclosed
	—
	Not disclosed
	Utilisation 8-10 MGD range. Midpoint 9 used. Near-full.

	
	
	Coronation Pillar NSTP 15 MGD
	15
	13.5
	90%
	Not disclosed
	—
	Not disclosed
	Utilisation 12-15 MGD range. Midpoint 13.5 used. Near-full.

	AGGREGATE TOTAL (All STPs)
	713.6
	601.51
	84.3%
	10 at 100% (31.3%) | 5 overloaded >100% (15.6%) | 17 underutilised <100% (53.1%)


 
Key Flags and Gaps
	Flag
	Division/STP
	Issue
	Implication

	OVERLOADED
	EE(SDW)-XIII / Yamuna Vihar 25 MGD
	28-29 MGD flow vs 25 MGD installed (112-116%). Dual-zone reporting conflict.
	Sewage bypassing treatment. Data manipulation risk between zones.

	SEVERE UNDERUSE
	EE(SDW)-III / Sonia Vihar WWTP
	Rs 55.70 Cr plant (2024) running at only 1.6% capacity.
	Capital already sunk; sewage still untreated elsewhere while new plant sits idle.

	SUSPECT O&M
	EE(SDW)-XIV / CWG Akshardham
	Identical O&M: Rs 83.76 L every year FY21-FY26. Zero variation across 5 years.
	Flat figures across 5 years without any variation suggest figures may be copied, not actual.

	DATA WITHHELD
	EE(SDW)-IV / Kondli (all 5 STPs)
	Detailed O&M, capital cost, commissioning data declared 'bulky'; applicant directed to visit office.
	114 MGD of capacity unverifiable. RTI obligation not met.

	DDA OWNERSHIP
	EE(SDW)-XIV / CWG Akshardham
	STP is DDA deposit work; DJB merely operates. Budget allocated by DDA.
	Accountability split between DDA and DJB. Reforms or upgrades require DDA approval.

	NEW PLANT UNDERPERFORMING
	EE(SDW)-II / Okhla 124 MGD
	Rs 1168 Cr plant (15% Delhi + 85% Centre) commissioned 2025, running at only 81%.
	Same pattern as Sonia Vihar: massive capital spent, plant underutilised from day one. 24 MGD idle.

	O&M SPIKE
	EE(SDW)-XI / Mehrauli STP
	O&M jumped from Rs 29.99 L (FY22) to Rs 131.19 L (FY23) — a 4x spike — then dropped to Rs 79.95 L and Rs 58.70 L. No explanation in RTI.
	Unexplained expenditure spike warrants audit. No CPCB/NGT penalty, but financial irregularity possible.

	THIRD-PARTY OPERATOR
	EE(SDW)-V / Delhi Gate Ph-I & SNH
	Both STPs maintained by PPCL, not DJB directly.
	Accountability and performance monitoring rests with contractor. DJB oversight critical.

	OKHLA IDLE CAPACITY
	EE(SDW)-II / Okhla 30 & 16 MGD
	Okhla 30 MGD at 43%; Okhla 16 MGD at 44%. Both over 50% idle. O&M data withheld as voluminous.
	Combined 26 MGD unused at established STPs. Financial waste compounded by withheld O&M data.

	O&M SPIKE — CRITICAL
	EE(SDW)-XII / Rohini STP
	O&M FY24 = Rs 7035 L (Rs 70.35 Cr) vs FY22 = Rs 264.42 L. A 27x spike in one year, then dropped to Rs 1385 L in FY25.
	Largest single-year O&M figure in dataset by far. Demands audit. No explanation in RTI. Budget utilisation only 62.5% overall despite the spike.

	DUAL-ZONE CONFLICT
	EE(SDW)-XII & EE(SDW)-IX / Rithala STP
	EE-XII claims Rithala STP (40 MGD) at 100%. EE-IX claims Rithala Ph-I (40 MGD) at 40.69 MGD (101.7%). Two divisions claiming same plant.
	Same pattern as Yamuna Vihar dual-zone conflict. Installed capacity effectively counted twice in aggregate. Real utilisation figure unclear.

	PLANT UNDER REHABILITATION
	EE(SDW)-IX / Rithala Ph-I
	O&M declared NIL for last 5 years — plant under rehabilitation. Yet utilisation reported at 40.69 MGD (101.7% overloaded).
	Overloaded plant with zero O&M spend for 5 years. Structural/operational integrity risk. Sewage being treated with no maintenance budget.

	POST-UPGRADE UNDERUSE
	EE(SDW)-VI / Keshopur Ph-III
	Capacity upgraded from 40 to 60 MGD (added 20 MGD). Actual utilisation only 32.17 MGD — 53.6% of new capacity.
	Upgrade investment wasted. 27.83 MGD idle post-expansion. No capital cost disclosed for the upgrade.

	OVERLOADED ×4
	Keshopur Ph-I / Nilothi-II / Yamuna Vihar / Coronation 20 MGD
	4 additional plants now confirmed overloaded: Keshopur Ph-I (107%), Nilothi-II (102.5%), Coronation 20 MGD (112.5%), plus existing Yamuna Vihar XIII (114%) and Rithala Ph-I (101.7%).
	Total 6 plants overloaded across dataset. Untreated sewage overflow systematic, not isolated.


 
Data Sources: RTI Act 2005. Responses received from: EE(SDW)-III (19.05.2026), EE(SDW)-XIII (13.05.2026), EE(SDW)-XIV (08.05.2026), EE(SDW)-IV/Kondli (11.05.2026), EE(SDW)-II/Okhla (batch 2), EE(SDW)-V/Andrews Ganj (batch 2), EE(SDW)-XI/Kilokri (batch 2), EE(SDW)-VI/Keshopur-Najafgarh (24.03.2026), EE(SDW)-XII/Rohini (28.03.2026), EE(SDW)-IX/Rithala Ph-I (12.03.2026), EE(SDW)-VII/Coronation Pillar (27.03.2026). EE(SDW)-I confirmed no STP under jurisdiction. NOTE: EE-VII utilisation figures reported as ranges; midpoints used for calculations. Rithala STP counted once in aggregate (EE-IX figure used); EE-XII claim flagged as duplicate.
